For 1990-2009 cars

#### Tools Required

• | J 2619-01 Slide Hammer

• | J 8092 Universal Drive Handle 3/4 Inch - 10

• | J 21426 Extension Housing Seal Installer

• | J 29369-2 Bushing and Bearing Remover 2-3 inch

• | J 45232 Differential Bearing Adjuster Needle Bearing Installer - Left

### Removal Procedure

1. Remove the wheel drive shaft. Refer to Wheel Drive Shaft Replacement .
2. Remove the swaybar link from the lower control arm. Refer to Stabilizer Shaft Link Replacement .
3. Using the J 29369-2 (2) and the J 2619-01 (1) , remove the axle seal.
4. Using the J 29369-2 (1) and the J 2619-01 (2) , remove the axle bearing.

### Installation Procedure

1. Position the axle bearing in the intermediate housing.
2. Using the J 45232 (1) and the J 8092 (2) , install the axle bearing.
3. Using the J 21426 (1) , install the axle seal.
4. Install the wheel drive shaft. Refer to Wheel Drive Shaft Replacement .
5. Install the swaybar link to the lower control arm. Refer to Stabilizer Shaft Link Replacement .
6. Check in fluid level. Refer to Front Axle Lubricant Level Inspection .
7. Lower the vehicle.