For 1990-2009 cars

Table 1: | Supplemental Inflatable Restraint Scan Tool Data Parameters
Table 2: | Supplemental Inflatable Restraint Scan Tool Output Controls

#### Supplemental Inflatable Restraint Scan Tool Data Parameters

Parameter | Expected Value | Definition
--- | --- | ---
Operating Conditions: Ignition ON
Active Switch | Enabled | The scan tool displays Enabled or Disabled. This is the state of the SIR active switch.
Active Switch | Not Present | The scan tool displays Present or Not Present. This is the state of the SIR active switch.
Battery Voltage Signal | Varies | This displays volts. This is the voltage input supplied to the SDM.
Driver Seat Belt Switch | Unbuckled | The scan tool displays Buckled or Unbuckled. This is the state of the driver seat belt.
Driver Seat Belt Switch | Not Present | The scan tool displays Present or Not Present. This is the state of the driver seat belt.
Driver Frontal Stage 1 Loop | Not Present | The scan tool displays Present or Not Present. This is the state of the driver front loop.
Driver Frontal Stage 2 Loop | Not Present | The scan tool displays Present or Not Present. This is the state of the driver front loop.
Driver Side Impact Sensor | Not Present | The scan tool displays Present or Not Present. This is the state of the driver side impact sensor.
Front End Sensor 1 | Not Present | The scan tool displays Present or Not Present. This is the state of the front end sensor 1.
Front End Sensor 2 | Not Present | The scan tool displays Present or Not Present. This is the state of the front end sensor 2.
Psgr. Frontal Stage 1 Loop | Not Present | The scan tool displays Present or Not Present. This is the state of the passenger front loop.
Psgr. Frontal Stage 2 Loop | Not Present | The scan tool displays Present or Not Present. This is the state of the passenger front loop.
Psgr. Side Impact Sensor | Not Present | The scan tool displays Present or Not Present. This is the state of the passenger impact sensor.
Passenger Seat Belt Switch | Unbuckled | The scan tool displays Buckled or Unbuckled. This is the state of the passenger seat belt.
Passenger Seat Belt Switch | Not Present | The scan tool displays Present or Not Present. This is the state of the passenger seat belt.
Passenger Presence System | Not Present | The scan tool displays Present or Not Present. This is the state of the passenger presence system.

#### Supplemental Inflatable Restraint Scan Tool Output Controls

Scan Tool Output Control | Description
--- | ---
Setup New SDM | This output control is used to set up a new SDM.
Setup SDM Part Number in BCM | This output control is used to set up a new SDM part number in the BCM.