For 1990-2009 cars

## Compressor Clutch Plate/Hub Assembly Replacement LLV, LLR

### Removal Procedure

1. Remove the compressor. Refer to Air Conditioning Compressor Replacement .
2. Remove the clutch plate retaining bolt (1).
3. Remove the clutch plate assembly (2).
4. Remove the clutch hub/bearing snap ring (3).
5. Remove the clutch hub/bearing assembly (4).

### Installation Procedure

1. Install the clutch hub/bearing assembly (4).
2. Install the clutch hub/bearing snap ring (3).
3. Install the clutch plate assembly (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the clutch plate retaining bolt (1).

Tighten
Tighten the bolt to 18 N·m (13 lb ft).

5. Install the compressor. Refer to Air Conditioning Compressor Replacement .