For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter Nut | 50 N·m | 37 lb ft
Exhaust Manifold Bolt

- First Pass

20 N·m

15 lb ft

- Second Pass

20 N·m

15 lb ft

- Final Pass

20 N·m

15 lb ft

Exhaust Manifold Heat Shield Nut | 10 N·m | 89 lb in
Heat Shield Nut | 9 N·m | 80 lb in
Leaf Spring Bolt and Nut | 85 N·m | 63 lb ft
Lower Shock Absorber Bolt and Nut | 95 N·m | 70 lb ft
Muffler Nut | 45 N·m | 33 lb ft
Transmission Filler Tube Bracket Nut | 12.5 N·m | 111 lb in