For 1990-2009 cars

### Removal Procedure

1. Remove the bolt securing the child seat restraint bracket to the vehicle.
2. Remove the child seat restraint bracket from the vehicle.

### Installation Procedure

1. Position the child seat restraint bracket by hooking the 2 tabs on the rear of the bracket into the slots in the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the bolt which retains the child seat restraint bracket to the vehicle.

Tighten
Tighten the child seat restraint bracket bolt to 52.5 N·m (39 lb ft).