For 1990-2009 cars

#### Tools Required

J 22912-B Split-Plate Bearing Puller

1. Remove the 4th gear blocking ring from the input shaft.
2. Remove the output shaft front support bearing from the input shaft.
3. Inspect the input shaft bearing for being faulty. Refer to Bearings and Spacers Cleaning and Inspection .
4. If the bearing is faulty, remove the input shaft bearing retaining ring.
5. Using a hydraulic press and J 22912-B , remove the input shaft bearing. Discard the bearing. Do not use the bearing after removal.