For 1990-2009 cars

#### Tools Required

EN-46745 Piston Pin Retainer Remover and Installer

Caution: Handle the piston carefully. Worn piston rings are sharp and may cause bodily injury.

Important: Do not reuse the piston rings.

1. Remove the piston rings using a piston ring expander.

Important: Two retainers hold the piston pins in place. Reuse the retainers if they are not damaged during removal.

2. Remove the piston pin retainers using EN-46745 .
3. Remove the piston pin.