For 1990-2009 cars

### Removal Procedure

1. Remove the jack stowage cover. Refer to Jack Stowage Cover Replacement.
2. Remove the jack from the stowage bracket by turning the jack handle to loosen the jack.
3. Remove the 2 bolts securing the jack stowage bracket to the vehicle.

### Installation Procedure

1. Position the jack stowage bracket on the floor stud in the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 bolts securing the jack stowage bracket to the vehicle. Tighten the jack stowage bracket bolts to 9 N·m (79 lb in).
3. Install the jack in the stowage bracket by positioning the jack on the 2 studs then turning the jack handle to tighten the jack in the bracket.
4. Install the jack stowage cover. Refer to Jack Stowage Cover Replacement.