For 1990-2009 cars

### Removal Procedure

1. Place your fingers as far as possible behind the mirror glass towards the center of the back.
2. Remove the mirror glass (1) from the mirror motor (2) with sufficient force to disengage the snap-locks on the mirror motor.
3. Remove the mirror glass from the mirror.

### Installation Procedure

1. Position the mirror glass (1) to the mirror motor (2).
2. Install the mirror glass to the mirror motor with the palm of the hand on the center of the glass, pressing in until fully seated.
3. Inspect the mirror for proper operation.