For 1990-2009 cars

### Removal Procedure

1. Remove the right hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Right Side .
2. Remove the blower motor mounting screws.
3. Remove the blower motor cooling tube (2).
4. Disconnect the blower motor electrical connector (4).
5. Remove the blower motor (3).

### Installation Procedure

1. Install the blower motor (3).
2. Connect the blower motor electrical connector (4).
3. Install the blower motor cooling tube (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the blower motor mounting screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

5. Install the right hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Right Side .