For 1990-2009 cars

### Removal Procedure

1. Remove the oil fill cap.
2. Grasp the front of the intake manifold sight shield and lift up disengaging the grommets from the studs.
3. Remove the intake manifold sight shield from the retainer slots.
4. Remove the intake manifold sight shield retainer bolts and retainer, if required.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Position the intake manifold sight shield on top of the intake manifold, aligning the holes, if required.
2. Install the intake manifold sight shield retainer bolts, if required.

Tighten
Tighten the bolts to 5 N·m (44 lb in).

3. Install the intake manifold sight shield tabs into the slots in the retainer.
4. Align the intake manifold sight shield grommets with the studs.
5. Gently push down on the intake manifold sight shield over the grommets, seating the intake manifold sight shield.
6. Install the oil fill cap.