For 1990-2009 cars

## Generator Bracket Replacement LH8

### Removal Procedure

1. Remove the generator. Refer to Generator Replacement.
2. Remove the power steering pump. Refer to Power Steering Pump Replacement.
3. Remove the drive belt idler pulley. Refer to Drive Belt Idler Pulley Replacement.
4. Remove the engine wiring harness bracket bolt (4).
5. Reposition the engine wiring harness bracket out of the way.
6. Remove the generator bracket bolts.
7. Remove the generator bracket.

### Installation Procedure

1. Install the generator bracket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the generator bracket bolts and tighten to 50 N·m (37 lb ft).
3. Position the engine wiring harness bracket to the generator bracket.
4. Install the engine wiring harness bracket bolt (4) and tighten to 40 N·m (29.5 lb ft).
5. Install the drive belt idler pulley. Refer to Drive Belt Idler Pulley Replacement.
6. Install the power steering pump. Refer to Power Steering Pump Replacement.
7. Install the generator. Refer to Generator Replacement.