For 1990-2009 cars

### Tools Required

• | J 25033-C Power Steering Pump Pulley Installer

• | J 25034-C Power Steering Pump Pulley Remover

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement for the 2.9L engine or Drive Belt Replacement for the 3.7L engine.
2. Remove the power steering pump pulley using J 25034-C .
3. Remove the pulley from the pump shaft.

### Installation Procedure

1. Install the power steering pump pulley to the end of the power steering pump shaft.
2. Install the power steering pump pulley to the power steering pump using J 25033-C .
3. Install the power steering pump pulley (1) flush against the end of the power steering pump shaft (2), with an allowable variance of 0.25 mm (0.010 in).
4. Install the drive belt. Refer to Drive Belt Replacement for the 2.9L engine or Drive Belt Replacement for the 3.7L engine.