For 1990-2009 cars

## Transmission Housing Oil Seal Replacement - Rear RWD

#### Tools Required

J 45868 RWD Output Shaft Seal Installer

### Removal Procedure

1. Remove the rear propeller shaft. Refer to One-Piece Propeller Shaft Replacement or Two-Piece Propeller Shaft Replacement .
2. Using a suitable tool, pry the rear transmission housing oil seal from the transmission housing.

### Installation Procedure

1. Using the J 45868 and a hammer, install the NEW rear transmission housing oil seal.
2. Check the transmission fluid level. Add if necessary. Refer to Transmission Fluid Replacement .
3. Install the rear propeller shaft. Refer to One-Piece Propeller Shaft Replacement or Two-Piece Propeller Shaft Replacement .

## Transmission Housing Oil Seal Replacement - Rear 4WD

#### Tools Required

• | J 6125-1B Slide Hammer

• | J 23129 Universal Seal Remover

• | J 45867 4WD Output Shaft Seal Installer

### Removal Procedure

1. Remove the transfer case assembly. Refer to Transfer Case Assembly Replacement .
2. Using the J 6125-1B (1) and J 23129 (2) remove the rear transmission housing oil seal from the housing.

### Installation Procedure

1. Using the J 45867 and a hammer, install the NEW rear transmission housing oil seal.
2. Check the transmission fluid level. Add if necessary. Refer to Transmission Fluid Replacement .
3. Install the transfer case assembly. Refer to Transfer Case Assembly Replacement .