For 1990-2009 cars

### Removal Procedure

1. Remove the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
2. Remove the upper anchor bolt for the front seat belt. Refer to Front Seat Belt Replacement .
3. Remove the seat belt adjuster knob.
4. Grasp the top of the upper center pillar trim panel and gently pull the panel away from the body to release the fasteners.
5. Remove any fasteners that may have pulled away from the panel and reinstall them to the back of the panel.
6. Remove the upper center pillar trim panel from the vehicle.

### Installation Procedure

1. Position the upper center pillar trim panel.
2. Ensure that the panel fasteners are aligned with the holes in the body.
3. Install the panel by pushing firmly against the body to seat the panel fasteners.
4. Install the seat belt adjuster knob.
5. Install the upper anchor bolt for the front seat belt. Refer to Front Seat Belt Replacement .
6. Install the lower center pillar trim panel. Refer to Center Pillar Lower Trim Panel Replacement .