For 1990-2009 cars

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. Use the J 25070 in order to heat the molding and the surrounding sheet metal to 82-93°C (180-200°F).
2. Remove the roof joint molding.

• | Use a flat-bladed tool in order to pry off the molding between the sealer and the joint. Use pliers or a similar tool in order to handle the hot molding and pull the molding loose. The molding and the sealer should come off in one piece.

• | Do not damage the paint on the cab.

3. Clean the joint in order to remove any remaining sealer. Sealer could interfere with the fit of the replacement molding.

### Installation Procedure

1. Use the J 25070 in order to heat the cab in the joint area. Preheat the sheet metal to approximately 93°C (200°F).
2. Install the molding.