For 1990-2009 cars

### Removal Procedure

Important: If removing both front power seats, remove the passenger seat first. Power to the passenger seat is terminated once the driver's seat is disconnected.

1. Ensure that the seat is all the way rearward.
2. Remove the bolt covers and front bolts.
3. Ensure that the seat is all the way forward.
4. Remove the rear bolts.
5. Disconnect the seat electrical connectors to the body harness.
6. Remove the seat from the vehicle.

### Installation Procedure

1. Position the seat in the vehicle.
2. Connect the seat electrical connectors to the body harness.
3. Install the rear bolts.
4. Ensure that the seat is all the way rearward.

Notice: Refer to Fastener Notice in the Preface section.

Important: After installation of a manual seat, move your body around in the seat to insure that the manual seat adjuster positively locks into position.

5. Install the front bolts.

Tighten
Tighten the front seat mounting bolts to 52.5 N·m (39 lb ft).

6. Install the bolt covers.