For 1990-2009 cars

### Removal Procedure

1. Remove the right front door sill plate. Refer to Front Side Door Sill Plate Replacement .
2. Remove the right hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Left Side .
3. Remove the instrument panel (I/P) compartment door. Refer to Instrument Panel Compartment Door Replacement .
4. Disconnect the radio antenna cable (1) from the extension cable.
5. Remove the grommet from the hinge pillar in an outbound direction.
6. Attach a mechanics wire to the to the antenna cable (1).
7. Remove the antenna mast. Refer to Fixed Antenna Mast Replacement .
8. Remove the screws retaining the antenna base.
9. Remove the grommet (1) and cable from the routing hole.
10. Remove the antenna cable from the vehicle.
11. Leave the mechanics wire in place for assembly purposes.

### Installation Procedure

1. Attach the mechanics wire to the end of the antenna cable.
2. Pull on the mechanics wire to route the cable and grommet (1) through the hinge pillar.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screws retaining the antenna base.

Tighten
Tighten the screws to 7.5 N·m (66 lb in).

4. Install the antenna mast. Refer to Fixed Antenna Mast Replacement .
5. Remove the mechanics wire from the antenna cable (1).
6. Install the grommet to the hinge pillar.
7. Connect the radio antenna cable (1) to the extension cable.
8. Install the I/P compartment door. Refer to Instrument Panel Compartment Door Replacement .
9. Install the right hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement - Left Side .
10. Install the right front door sill plate. Refer to Front Side Door Sill Plate Replacement .