For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
2. Remove the fasteners retaining the switch to the trim plate.
3. Remove the switch from the trim plate.

### Installation Procedure

1. Install the switch to the trim plate.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the fasteners retaining the switch to the trim plate.

Tighten
Tighten the fastener to 2.5 N·m (22 lb in).

3. Install the I/P accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .