For 1990-2009 cars

### Removal Procedure

1. Remove the battery. Refer to Battery Replacement .
2. Disconnect the following from the lower battery box (2):

• | The battery cables harness retainer (3)

• | The engine wiring harness retainer

3. Lift the lower battery box (2) upward from the battery tray (3).

### Installation Procedure

1. Install the lower battery box (2) to the retainer stud (1) and battery tray (3).
2. Connect the following to the lower battery box (2):

• | The battery cables harness retainer (3)

• | The engine wiring harness retainer

3. Install the battery. Refer to Battery Replacement .