For 1990-2009 cars

1. Inspect the transmission wiring harness assembly (224) for the following:

• | Cut or pinched wires

• | Cut wire insulation

• | Bent or broken electrical connectors

2. Position the wire harness assembly (224) onto the valve body and pump assembly.
3. Mate each connector to its respective electrical component. Engage the locking tabs.
4. Secure the harness conduit into the retaining clips (225, 226).
5. Insert the automatic transmission temperature sensor (391) into the retaining clip (390).