For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 8A (REV. INFORMATION BY PAGE NO.)

********************************************************************** SERVICE MANUAL UPDATE SECTION 8A **********************************************************************

PLEASE MAKE THE FOLLOWING CHANGES TO THE OLDSMOBILE "N" CAR SERVICE MANUAL:

PAGE ZONE REVISION CATEGORY REVISION **** **** ***************** ********

8A-14-3 F LATE PRODUCTION CHANGE THE CONNECTOR LABEL ON THE BRAKE FLUID LEVEL SWITCH FROM B TO A.

8A-34-10 E REVISED CHANGE THE THIRD STATEMENT ON THE FIRST BOX TO: JUMPER TERMS "A" AND "E" OF CRUISE CONTROL SERVO TO BATTERY VOLTAGE.

8A-41-0 A,B LATE PRODUCTION THE TAN/WHT (33) WIRE ALWAYS CONNECTS TO TERMINAL B OF THE BRAKE FLUID LEVEL SWITCH CONNECTOR (DELETE A AND THE ASTERISKS).

THE BLK (150) WIRE ALWAYS CONNECTS TO TERMINAL A OF THE BRAKE FLUID LEVEL SWITCH CONNECTOR (DELETE B AND THE ASTERISKS).

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1992 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.