For 1990-2009 cars

Table 1: | Electronic Brake Control Module
Table 2: | Instrument Panel Cluster -- Buick And Oldsmobile
Table 3: | Instrument Panel Cluster -- Pontiac Only
Table 4: | C1 Remote Control Door Lock Receiver

#### Electronic Brake Control Module

Connector Part Information |

• | 12160423

• | 32-Way F Metri-Pack Series 280 Micro-Pack Series 100 W (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRA | 1056 | Steering Wheel Position Sensor Feed - 5 Volt Reference
2 | PNK | 1632 | ABS Enable Relay Output - Coil
3 | GRN DK | 1288 | ABS Isolation Solenoid Feed - Left Front
4 | PNK | 439 | Fuse Output - Ignition 1 - Type III Fuse
5 | ORN/BLK | 556 | Steering Wheel Position Sensor Return
8 | BLU LT | 830 | Wheel Speed Sensor Signal - Left Front
9 | GRN DK | 872 | Wheel Speed Sensor Signal - Right Front
10 | BLK | 884 | Wheel Speed Sensor Signal - Left Rear
11 | BRN | 882 | Wheel Speed Sensor Signal - Right Rear
12 | TAN | 800 | Serial Data Signal - UART - 8192 Baud - Primary
13 | ORN | 340 | Fuse Output - Battery - Type III Fuse
16 | WHT | 17 | Stop Lamp Switch Output
17 | BLU LT | 1059 | Steering Wheel Position Sensor Signal
18 | BRN | 1295 | Electronic Variable Orifice Solenoid Output
19 | BLU LT | 1289 | ABS Isolation Solenoid Feed - Right Front
20 | PNK | 849 | Brake Fluid Level Sensor Signal
21 | YEL | 873 | Wheel Speed Sensor Return - Left Front
22 | TAN | 833 | Wheel Speed Sensor Return - Right Front
23 | RED | 885 | Wheel Speed Sensor Return - Left Rear
24 | WHT | 883 | Wheel Speed Sensor Return - Right Rear
A | PPL | 1282 | ABS Motor Feed - Right Front
B | BLK | 1283 | ABS Motor Return - Right Front
C | RED | 1633 | ABS Enable Relay Output - N.O Contact
D | BLK | 250 | Ground
E | ORN | 1285 | ABS Motor Return - Rear
F | GRN DK | 1284 | ABS Motor Feed - Rear
G | BLK | 1280 | ABS Motor Feed - Left Front
H | PNK | 1281 | ABS Motor Return - Left Front

#### Instrument Panel Cluster -- Buick And Oldsmobile

Connector Part Information |

• | 12045575

• | 32-Way F Micro-Pack Series 100 Instrument Panel Cluster (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | GRA | 8 | Instrument Panel Lamp Feed
C2 | -- | -- | Not Used
C3 | WHT | 1459 | Magnetic Rotation Detection Ignition Key Cylinder Sensor Feed -12 Volt Reference
C4 | -- | -- | Not Used
C5 | YEL | 1836 | Magnetic Rotation Detection Sensor Signal
C6 | BLK | 1835 | Magnetic Rotation Detection Sensor Return
C7 | BLK | 1350 | Ground
C8 | TAN | 800 | Serial Data Signal - UART - 8192 BAUD - Primary
C9 | -- | -- | Not Used
C10 | BLK | 150 | Ground
C11 | PNK | 1020 | Fuse Output - Off, Run, Crank - Type III Fuse
C12 | WHT | 991 | Automatic Lamp Control Relay Ground
C13 | GRN LT/BLK | 592 | Daytime Running Lamp Relay Output - Coil
C14 | ORN | 1440 | Fuse Output - Battery - Type III Fuse
C15 | BLK/WHT | 451 | Engine Control Module Ground
C16 | BLU LT | 1134 | Park Brake Switch Signal
D1 | PPL | 30 | Fuel Gage Sensor Signal
D2 | GRN LT | 11 | High Beam Headlamp Feed
D3 | TAN | 12 | Low Beam Headlamp Feed
D4 | GRN DK/WHT | 817 | Vehicle Speed Signal - 4000 Pulses/Mile
D5-D6 | -- | -- | Not Used
D7 | BLU DK | 15 | Turn Signal Lamp Feed - Right Front
D8 | BLU LT | 15 | Turn Signal Lamp Feed - Left Front
D9 | BRN/WHT | 419 | Check Engine Indicator Lamp Output
D10 | -- | -- | Not Used
D11 | GRN LT | 66 | Air Conditioning Switch Output
D12-D13 | -- | -- | Not Used
D14 | BRN/WHT | 1571 | Traction Control System Switch Signal
D15 | -- | -- | Not Used
D16 | TAN | 185 | Low Windshield Washer Fluid Indicator Lamp Output

#### Instrument Panel Cluster -- Pontiac Only

Connector Part Information |

• | 12045575

• | 32-Way F Micro-Pack Series 100 Instrument Panel Cluster (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | BLK | 1350 | Ground
C2 | LT GRN | 11 | High Beam Headlamp Feed
C3 | YEL | 1836 | Magnetic Rotation Detection Sensor Signal
C4 | -- | -- | Not Used
C5 | PPL | 30 | Fuel Gauge Sensor Signal
C6 | RED | 1789 | Catalytic Converter Temperature Sensor Signal
C7-C9 | -- | -- | Not Used
C10 | PNK | 1020 | Fuse Output - Off, Run, Crank -Type III Fuse
C11 | LT GRN/BLK | 592 | Daytime Running Lamp Relay Output - Coil
C12 | WHT | 991 | Automatic Lamp Control Relay Ground
C13 | -- | -- | Not Used
C14 | ORN | 1440 | Fuse Output - Battery - Type III Fuse
C15 | -- | -- | Not Used
C16 | GRY | 8 | Instrument Panel Lamp Feed
D1 | -- | -- | Not Used
D2 | TAN | 12 | Low Beam Headlamp Feed
D3 | DK GRN/WHT | 817 | Low Beam Headlamp Feed
D4 | WHT | 1459 | Magnetic Rotation Detection Device 12-Volt Feed
D5 | TAN | 800 | Serial Data Signal - UART - 8192 BAUD - Primary
D6 | BLU DK | 15 | Turn Signal Lamp Feed - Right Front
D7 | LT BLU | 14 | Turn Signal Lamp Feed - Left Front
D8 | BRN/WHT | 419 | Check Engine Indicator Lamp Output
D9 | -- | -- | Not Used
D10 | BRN/WHT | 1571 | Traction Control Switch Signal
D11 | LT BLU | 1134 | Park Brake Switch Signal
D12 | BLK | 1835 | Magnetic Rotation Detection Sensor Return
D13 | BLK/WHT | 451 | Engine Control Module Ground
D14 | LT GRN | 66 | A/C Switch Output
D15 | BLK | 150 | Ground
D16 | -- | -- | Not Used

#### C1 Remote Control Door Lock Receiver

Connector Part Information |

• | 12129431

• | 16-Way F Metri-Pack Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 694 | Power Door Lock Motor Feed-Driver Door Unlock
B | WHT | 194 | Power Door Lock Relay Feed-Unlock Coil
C | -- | -- | Not Used
D | -- | -- | Not Used
E | ORN | 40 | Fuse Output-Battery-Type III Fuse
F | -- | -- | Not Used
G | BLK/WHT | 56 | Trunk Release Motor Feed
H | -- | -- | Not Used
J | PNK | 39 | Fuse Output-Ignition 1-Type III Fuse
K | WHT/BLK | 572 | Keyless Entry Enable Signal
L | BLK/WHT | 1455 | Keyless Entry Program Enable Signal
M | -- | -- | Not Used
N | BLK | 150 | Ground
P | -- | -- | Not Used
R | LT BLU | 195 | Power Door Lock Relay Feed-Lock Coil
S | WHT | 156 | Courtesy Light Output