For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 6627-A Wheel Stud Remover

• | J 28733-A Front Hub Spindle Remover

1. Remove the hub and bearing assembly.
2. Remove the wheel stud (1) from the hub and bearing assembly using the J 6627-A . Discard the stud.

### Installation Procedure

1. Install the new wheel stud into the hub and bearing assembly (2).
2. Install the four flat washers (3) and the stud (flat side down) onto the wheel stud, and tighten the nut (1) until the wheel stud is fully seated.
3. Install the hub and bearing assembly (2). Refer to Front Wheel Bearing and Hub Replacement .
4. Check the front wheel alignment. Refer to Wheel Alignment Specifications