For 1990-2009 cars

### Removal Procedure

Important: If you need to use pliers in order to twist the tilt lever, use locking pliers with a piece of rubber between the jaws. The rubber will prevent damage to the tilt lever.

1. Grip the tilt lever (4) firmly.
2. Twist the tilt lever (4) counterclockwise in order to remove the lever

### Installation Procedure

1. Apply LOCTITE™ #201 or the equivalent to the threads.
2. Install the tilt lever (4). Twist the lever clockwise.