For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for a worn or damaged wheel bearing. Refer to Diagnosis in Steering, Suspension, Tires and Wheels. Are any of the wheel bearings worn or damaged? | -- | Go to Step 2 | Go to Step 3
2 | Service or replace the faulty wheel bearing. Did the vibration stop? | -- | System OK | Go to Step 3
3 | Check for a worn or damaged drive axle joint. Refer to Drive Axle Replacement in Drive Axle. Is a drive axle joint worn or damaged? | -- | Go to Step 4 | Go to Step 5
4 | Repair or replace the faulty drive axle joint. Refer to Wheel Drive Shaft Outer Joint and Boot Replacement in Wheel Drive Shafts. Did the vibration stop? | -- | System OK | Go to Step 5
5 |

1. Check for out of round tires. Refer to Tires and Wheels.
2. Add air to or replace tires.

Did the vibration stop?

--

System OK

Go to Step 6

6 |

1. Check for tire unbalance. Refer to Balancing Tire and Wheel in Tires and Wheels.
2. Rotate or service tires.

Did the vibration stop?

--

System OK

Go to Step 7

7 | Check for worn drive axle C/V joint. Refer to Outer C/V Joint and Seal Assembly in Drive Axle Unit Repair. Is the joint worn or damaged? | -- | Go to Step 8 | Go to Step 9
8 | Repair or replace the C/V joint. Did the vibration stop? | -- | System OK | Go to Step 9
9 |

1. Check for correct drive axle trim height. Refer to Vibrations in Steering, Suspension, Tire and Wheel Diagnosis.
2. Adjust trim height as necessary.

Did the vibration stop?

--

System OK

Go to Noisy in All Gears