For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Transaxle makes "clicking" noise on turns
1 | Check for a worn drive axle outboard C/V joint. Refer to Outer C/V Joint and Seal Assembly in Drive Axle Unit Repair. Is the joint worn? |  | Go to Step 2 | Refer to Noisy in All Gears
2 | Replace the CV joint. Did the noise disappear? |  | System OK | Refer to Noisy in All Gears