For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement in Bumpers.
2. Remove the nuts (1) that retain the rear end panel (2) to the striker (3).
3. Remove the striker (3).

### Installation Procedure

1. Install the striker (3) to the rear end panel (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the nuts (1) that retain the rear end panel (2) to the striker (3).

Tighten
Tighten the nuts to 14 N·m (11 lb ft).

3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement in Bumpers.