For 1990-2009 cars

#### Tools Required

J 5403 Snap Ring Pliers

1. Coat the O-rings with 525 viscosity refrigeration oil.
2. Using thumb pressure, push the O-rings in place.

Important: Seat the retaining ring properly in the ring groove.

3. Using the J 5403 , install the valve retaining ring with the high point of the curved sides against the valve housing.
4. Evacuate the system. Recharge the system.
5. Perform a leak test. Refer to Compressor Leak Testing .