For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof window (13). Refer to Sunroof Window Height and Opening Fit Adjustment .
2. Remove the entire weather-strip (1) by pulling away from the window.

### Installation Procedure

1. On the passenger side of the vehicle, align the butt joint with the center of the sunroof window.
2. Work the weather-strip (1) into the channel in the window frame. Continue until the weather-strip is firmly pressed into the channel around the entire sunroof window.
3. Install the sunroof window (13). Refer to Sunroof Window Height and Opening Fit Adjustment .