For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment.
2. Remove the rear trim.
3. Remove the 4 wing nuts in order to remove the tail light lens assembly
4. Remove the tail light socket from the lens assembly.
5. Remove the bulb from the socket.

### Installation Procedure

1. Install the tail light bulb into the socket.
2. Install the socket into the lens assembly.
3. Use the 4 wing nuts in order to install the tail lamp lens assembly to the vehicle.
4. Install the rear trim.
5. Close the rear compartment.