For 1990-2009 cars

## Rear Bumper Fascia Molding Replacement Buick

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
2. Remove the retaining nuts.
3. Remove the molding from the rear fascia.

### Installation Procedure

1. Install the molding to the holes in the rear fascia.
2. Install the retaining nuts.
3. Install the rear fascia.

## Rear Bumper Fascia Molding Replacement Pontiac

### Removal Procedure

1. Warm the molding (3) to a temperature of 35-38°C (95-100°F) in order to ease the removal of the molding.
2. Pull out the end of the molding (3) and peel the molding from the fascia (2) in order to remove the molding.

### Installation Procedure

1. Warm the molding (3) to a temperature of 35-38°C (95-100°F).
2. Align the molding (3) to the fascia (2).
3. Peel the paper backing from the molding (3).
4. Place the end of the molding (3) into the fascia slot (1). Apply pressure in order to secure the molding.