For 1990-2009 cars

Important:

• | Only use oil free compressed air to blow out the fuel pipes.

• | Inspect the fuel tank internally and clean the fuel tank if you find a plugged fuel filter.

1. Relieve the fuel system pressure. Refer to the Fuel Pressure Relief Procedure
2. Drain the fuel tank. Refer to Fuel Tank Draining Procedure
3. Remove the fuel tank. Refer to Fuel Tank Replacement
4. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement
5. Inspect the fuel pump strainer. Replace a contaminated strainer and inspect the fuel pump.
6. Inspect the fuel pump inlet for dirt and debris. Replace the fuel pump if you find dirt or debris in the fuel pump inlet.
7. Flush the fuel tank with hot water.
8. Pour the water out of the fuel sender assembly opening. Rock the tank to be sure that removal of the water from the tank is complete.
9. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement
10. Install the fuel tank. Refer to Fuel Tank Replacement
11. Refill the fuel tank.
12. Install the fuel filler cap.
13. Connect the negative battery cable.
14. Inspect for fuel leaks through the following steps:

14.1. | Turn the ignition to the ON position for two seconds.

14.2. | Turn the ignition to the OFF for ten seconds.

14.3. | Turn the ignition to the ON position.

14.4. | Check for fuel leaks.