For 1990-2009 cars

### Disassembly Procedure

#### Tools

J 21854-01 Pivot Pin Remover

1. Remove the upper tilt head components assembly. Refer to Steering Column Tilt Head Housing - Disassemble - Off Vehicle .
2. Remove the ignition switch assembly. Refer to Ignition Switch Assembly - Disassemble - Off Vehicle .
3. Remove the ignition lock housing assembly. Refer to Lock Housing Assembly - Disassemble - Off Vehicle .
4. Remove the tilt spring. Refer to Tilt Spring - Disassemble - Off Vehicle .
5. Remove the 2 pivot pins using J 21854-01 .
6. Remove the bearing and housing assembly.