For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the map pocket nuts (2).
3. Remove the map pocket (1).

### Installation Procedure

1. Install the map pocket (1) by aligning the stud on the map pocket to the holes in the door trim panel.
2. Install the map pocket nuts (2).
3. Install the door trim panel. Refer to Door Trim Panel Replacement .