For 1990-2009 cars

1. Cover adjacent areas of the panels with masking tape in order to protect the surface.
2. Determine if any of the screws, bolts or clips allow water to enter the interior of the body. Use one of the following items in order to seal the leaks:

• | Body caulking compound

• | Presealed screws, nuts or clips

3. Do not use rotating adhesive removal discs on the molding. These discs generate excessive heat. Excessive heat may damage the molding.