For 1990-2009 cars

### Removal Procedure

1. Remove the composite headlamp assembly. Refer to Headlamp Assembly Replacement .
2. Twist the turn/park lamp socket counter-clockwise in order to remove the socket from the assembly.
3. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Twist the socket counter-clockwise in order to install the socket to the headlamp assembly.
3. Install the headlamp assembly. Refer to Headlamp Assembly Replacement .