For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 8A (REV. INFORMATION BY PAGE NO.)

#### SUBJECT: SMU - SECTION 8A (REVISED INFORMATION BY PAGE NUMBER)

#### VEHICLES AFFECTED: 1992 "N" MODEL - OLDSMOBILE ACHIEVA

SERVICE MANUAL UPDATE SECTION 8A

- - - - - - - - - - -

Please make the following changes to the Oldsmobile Achieva "N" Car Service Manual:

Page Zone Revision Category Revision ---- ---- ----------------- -------- 8A-14-3 F Late Production Change the connector label on the Brake Fluid Level Switch from B to A.

8A-34-10 E Revised Change the third statement on the first box to: Jumper terms "A" and "E" of Cruise Control Servo to battery voltage.

8A-41-0 A, B Late Production The TAN/WHT (33) wire always connects to terminal B of the Brake Fluid Level Switch connector (delete A and the asterisks).

The BLK (150) wire always connects to terminal A of the Brake Fluid Level Switch connector (delete B and the asterisks).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.