For 1990-2009 cars

# SMU-SEC. 7A REVISED PARK/ NEUTRAL POSITION SWITCH

#### SUBJECT: REVISED PARK/NEUTRAL POSITION SWITCH REMOVAL AND INSTALL PROCEDURE

MODEL/YEARS: 1992-93 ACHIEVA WITH THE 3300 ENGINE AND 3T40 TRANSAXLE

This bulletin replaces the "Park/Neutral Position Switch" procedure in Section 7A of the 1992 and 1993 service manuals.

The following procedure should be used:

#### Remove or Disconnect

1. Raise vehicle and suitably support, refer to Section OA.

2. Lower heater pipe bracket bolt.

3. Position vacuum hose aside.

4. Lower vehicle.

5. Pry off shift linkage.

6. Electrical connectors.

7. Park neutral position switch.

#### Install or Connect

1. Park/neutral position switch.

2. Electrical connector.

3. Shift linkage.

4. Raise vehicle.

5. Vacuum hose.

6. Lower heater pipe bracket bolt.

7. Lower vehicle.

Labor Operation Number: J6383

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.