For 1990-2009 cars

# WRONG FLUID LEVEL INDICATOR READS OVER/UNDER FULL (INFO)

#### SUBJECT: INCORRECT FLUID LEVEL INDICATOR READS OVERFULL OR UNDERFULL (INFORMATION)

VEHICLES AFFECTED: 1992 "N" MODEL WITH 2.3L ENGINE (VIN 3, A/RPO L40, LGO) AND 5 SPEED MANUAL TRANSAXLE

#### APPLICATION:

YEAR/MODEL: 1992 Pontiac and Oldsmobile "N" Car ENGINE: 2.3L (VIN 3) L40 2.3L (VIN A) LGO TRANSAXLE: ISUZU (M32) and NVG-T550 (MV5) 5 Speed Manual

#### SERVICE INFORMATION:

Some Isuzu 5 speed manual transaxles or NVG-T550 5 speed manual transaxles may show an extreme overfill or underfill condition on the fluid level indicator. The incorrect fluid level indicator may have been installed in the transaxle.

The Isuzu 5 speed manual transaxle should have a fluid level indicator with a WHITE handle. The NVG-T550 manual transaxle should have a fluid level indicator with a RED handle. Check for the proper colour coded indicator before draining or adding fluid to correct an overfull or underfull condition.

Replace fluid level indicator, if it does not have a RED handle with P/N 24572124.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.