For 1990-2009 cars

1. Turn the steering wheel so that the vehicle's wheels are pointing straight ahead.
2. Turn the ignition switch to the LOCK position.
3. Remove the key from the ignition switch.

Important: With the AIR BAG Fuse removed and the ignition switch in the RUN position, the AIR BAG warning lamp illuminates. This is a normal operation and does not indicate an SIR system malfunction.

4. Remove the AIR BAG Fuse from the fuse block.
5. Remove the Connector Position Assurance (CPA) from the driver yellow 2-way connector (1) located near the base of the steering column.
6. Disconnect the driver yellow 2-way connector (1) located at the base of the steering column.
7. Remove the I/P sound insulator (RH). Refer to Instrument Panel Insulator Replacement in Instrument Panel, Gauges and Console.
8. Remove the Connector Position Assurance (CPA) (2) from the passenger yellow 2-way connector (3) located under the RH I/P.
9. Disconnect the passenger yellow 2-way connector (1) located under the RH I/P.