For 1990-2009 cars

# SMU - SECTION 8A - REVISED COLOR DESIGNATIONS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 8A - REVISED COLOR DESIGNATIONS FOR FUSIBLE LINKS A, B, C

#### MODELS: 1995 BUICK SKYLARK 1995 OLDSMOBILE ACHIEVA 1995 PONTIAC GRAND AM

THIS BULLETIN IS BEING ISSUED TO REVISE THE COLOR DESIGNATIONS FOR FUSIBLE LINKS A, B, C REFERENCED ON THE FOLLOWING PAGES IN SECTION 8A OF THE SERVICE MANUAL.

FUSIBLE LINK A SHOULD BE CHANGED FROM .35 RUST TO .35 GRY (V6 VIN M) ON PAGE 8A-10-0.

FUSIBLE LINK B SHOULD BE CHANGED FROM 1 RUST TO 1 BLK ON PAGES 8A-10-0, 8A-30-0, 8A-30-1 AND 8A-63-0.

FUSIBLE LINK C SHOULD BE CHANGED FROM 2 RUST TO 2 GRY ON PAGES 8A-10-0 AND 8A-44-1.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.