For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disconnect the clutch actuator cylinder line.
3. Remove the transmission. Refer to Transmission Replacement in Manual Transmission - M5 and M7.
4. Remove the clutch actuator cylinder from the transmission.

### Installation Procedure

1. Lubricate the inside diameter of the bearing with GM P/N 12345777, or equivalent.
2. Install the clutch actuator cylinder to the transmission.
3. Install the transmission. Refer to Transmission Replacement in Manual Transmission - M5 and M7.
4. Connect the clutch actuator cylinder line.
5. Bleed the hydraulic system. Refer to Hydraulic Clutch Bleeding .
6. Connect the negative battery cable.