For 1990-2009 cars

# REAR WHEEL BRAKE DRAG (DIAGNOSE/REPLACE PARKING)

#### SUBJECT: REAR WHEEL BRAKE DRAG (DIAGNOSE/REPLACE PARKING BRAKE CABLES)

#### MODELS: 1995 BUICK SKYLARK 1995 OLDSMOBILE ACHIEVA 1995 PONTIAC GRAND AM

#### VIN BREAKPOINTS:

BUICK: PRIOR TO VIN SC411323 OLDSMOBILE: PRIOR TO VIN SM313630 PONTIAC: PRIOR TO VIN SC734169 (C PLANT) PRIOR TO VIN SM529184 (M PLANT)

#### CONDITION:

SOME OWNERS MAY COMMENT ON A REAR WHEEL BRAKE DRAG THAT IS MORE THAN DESIRABLE. HOWEVER, IT IS ACCEPTABLE TO HAVE ONE HIGH SPOT THAT DOES NOT REDUCE THE WHEEL FROM ROTATING FREELY.

#### CAUSE:

SOME PARKING BRAKE CABLE RETURN SPRINGS MAY LACK ENOUGH TENSION TO COMPLETELY RETURN THE PARK BRAKE LEVER WITHIN THE BRAKE ASSEMBLY.

#### CORRECTION:

FOLLOW THE PROCEDURE BELOW TO DETERMINE IF REPLACING THE PARKING BRAKE CABLE IS NECESSARY.

1. WITH ENGINE RUNNING, DEPRESS AND HOLD THE SERVICE BRAKE ON WITH MODERATE TO HEAVY APPLY FORCE.

2. WHILE SERVICE BRAKE IS APPLIED, CYCLE PARK BRAKE LEVER FOUR (4) TIMES. APPLY LEVER TO A MINIMUM OF 3/4 OF TRAVEL, (10) CLICKS MINIMUM.

3. RELEASE PARK BRAKE THEN RELEASE THE SERVICE BRAKE.

4. TURN ENGINE OFF.

5. WITH BOTH REAR WHEELS OFF THE GROUND, HAND TURN REAR WHEELS IN THE FORWARD DIRECTION AND OBSERVE THE AMOUNT OF WHEEL SPIN.

6. IF WHEEL SPINS FREELY (MAY HAVE ONE HIGH SPOT WHICH DOES NOT REDUCE THE WHEEL FROM ROTATING) - PARK BRAKE SYSTEM OK, NO FURTHER ACTION REQUIRED.

7. IF WHEEL DOES NOT SPIN FREELY, REPLACE BOTH PARKING BRAKE CABLES WITH P/N 22646659 (2 REQUIRED).

8. IF REAR SHOE TO DRUM CLEARANCE IS QUESTIONED, REFER TO SECTION 5C OF THE SERVICE MANUAL.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: H9995 (FOR DIAGNOSIS, OWNER CONCERN NOT DUPLICATED) LABOR TIME: 0.5 HRS.

LABOR OPERATION NUMBER: H2887 (FOR REPLACEMENT OF BOTH RIGHT AND LEFT CABLES) USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.