For 1990-2009 cars

#### Tools Required

• | J 38122-A Crankshaft Balancer Holder

• | J 24420-B Crankshaft Balancer Puller

Important: An automatic transmission crankshaft balancer must not be installed on a manual transmission equipped engine. A manual transmission crankshaft balancer must not be installed on an automatic transmission equipped engine.

1. Remove the balancer retaining bolt and washer. Use the J 38122-A in order to prevent the crankshaft from rotating when loosening the bolt.
2. Remove the balancer assembly. Use the J 24420-B .