For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
Balance Shaft Cover Nut and Bolt | 13 | -- | 115
Balance Shaft Driven Sprocket Bolt (left hand thread) | 30 + 45° | 22 + 45° | --
Balance Shaft to Housing Bolts 8 mm hex plus 45° | 10 | 11 | --
Balance Shaft Housing Bolts 10 mm hex plus 40° | 15 | 11 | --
Balance Shaft to block Bolts 13 mm hex | 25 | 18 | --
Balance Shaft to block Bolts 15 mm hex | 53 | 39 | --
Balance Shaft to Block Bolts 18 mm hex | 40 + 60° | 30 + 60° | --
Camshaft (exhaust) Rear Cover | 14 | -- | 124
Camshaft Position Sensor Bolt | 10 | -- | 89
Camshaft Sprocket to the Camshaft Bolt | 70 | 52 | --
Connecting Rod Nuts | 25 + 80° | 18 + 80° | --
Coolant Bleeder Valve | Fully Driven, Seated , Not Stripped
Coolant Outlet to Cylinder Head | 26 | 19 | --
Coolant Pump to the Timing Chain Housing | 26 | 19 | --
Coolant Pump to the Coolant Pump Cover | 14 | -- | 124
Coolant Pump Cover to the Block | 26 | 19 | --
Crankshaft Balancer to the Crankshaft | 175 + 90° | 129 + 90° | --
Crankshaft Bearing Cap Bolts | 20 + 90° | 15 + 90° | --
Crankshaft Position Sensor to Block | 9 | -- | 80
Cylinder Head Bolts | Refer to Procedure
Cylinder Head Threaded Plug | 26 | 19 | --
EGR Pipe to the EGR Adapter | 26 | 19 | --
Engine Coolant Air Bleed Pipe | 14 | -- | 124
Engine Coolant Air Bleed Pipe Nut | 42 | 31 | --
Engine Coolant Temperature Sensor to the Coolant Outlet | 11 | -- | 97
Engine Coolant Temperature Gauge Sensor to the Cylinder Head | Fully Driven, Seated, Not Stripped
Engine Lift Bracket | 96 | 68 | --
Engine To Transaxle Bolts (Long Bolts) | 100 | 74 | --
Engine To Transaxle Bolts (Short Bolt) | 58 | 43 | --
Engine To Transaxle Nut | 58 | 43 | --
Engine To Transaxle Stud | 12 | -- | 106
Engine Mount Bracket Adapter to Block Bolt for Manual Trans | 110 + 90° | 81+ 90° | --
Engine Mount Bracket Adapter to Block Bolt for AutoTrans | 60 + 90° | 44 + 90° | --
Engine Mount (right hand side) to the Engine Mount Bracket Bolts | 62 | 46 | --
Engine Mount (right hand side) to the Body Support Nut | 44 | 32 | --
Engine Mount (right hand side) to the body support bolt | 66 | 49 | --
Engine Mount Strut | 102 | 88 | --
Engine Mount Strut Bracket Front Bolts | 75 | 55 | --
Engine Mount Strut Bracket Bottom Bolts | 130 | 96 | --
EVAP Canister Purge Valve Solenoid Bracket Bolt | 8 | -- | 72
Exhaust Manifold Upper Heat Shield to the Manifold Bolts | 14 | -- | 124
Exhaust Manifold to the Cylinder Head Nuts | 15 | -- | 11
Exhaust Manifold to the Cylinder Head Studs | 11 | -- | 97
Exhaust Manifold Brace to the Exhaust Manifold Bolt | 56 | 41 | --
Exhaust Manifold Brace to the Oil Pan Nuts | 26 | 19 | --
Flywheel to Clutch Cover | 20 + 45° | 15 + 45° | --
Flywheel to the Converter | 63 | 46 | --
Flywheel to the Crankshaft | 30 + 45° | 22 + 45° | --
Front Cover to the Timing Chain Housing | 12 | -- | 106
Fuel Pipe Bracket to the Camshaft Housing | 15 | 11+30° | --
Fuel Pipe to the Fuel Rail Nut | 30 | 22 | --
Fuel Rail to the Camshaft Housing | 26 | 19 | --
Ignition Coil and Module Assembly to the Camshaft Housings | 22 | 16 | --
Intake Manifold to the Cylinder Head Bolts/Nuts | 24 | 19 | --
Intake Manifold to the Cylinder Head Studs | 11 | -- | 97
Knock Sensor | 20 | 15 | --
Oil Filter Connector to the Block | 29 | 21 | --
Oil/Air Separator To Block bolts | 24 | 19 | --
Oil Dipstick Tube nut | 8 | -- | 71
Oil Filter to the Block | 3/4 to one complete turn after gasket contact
Oil Pan Bolts | 24 | 17 | --
Oil Pan Bolts, Second Set | 12 | -- | 106
Oil Presssure Switch | 13 | -- | 115
Oil Pan Drain Plug | 26 | 19 | --
Oil Pan Studs | 26 | 19 | --
Oil Passage Plugs, Block 1/8x27 | 10 | -- | 89
Oil Passage Plugs, 3/8x18 | 30 | 22 | --
Oil Passage Plugs, 1/4x18 | 20 | 15 | --
Oil Passage Plug Bolt | 30 | 22 | --
Oil Pump Cover to the Balance Shaft Housing - Long Bolts | 12 | -- | 106
Oil Pump Cover to the Oil Pump Housing - Short Bolt | 10 | -- | 89
Oxygen Sensor to Exhaust Manifold | 42 | 31 | --
Powersteering Pipe to the Pump Nut | 27 | 20 | --
Powersteering Pump to the Cam Carrier Bolts | 26 | 19 | --
Rear Crankshaft Seal Housing to Block | 12 | -- | 106
Spark Plugs to the Cylinder Head | 18 | 13 | --
Starter Bolts | 90 | 66 | --
Tensioner to Tensioner Bracket Nut | 54 | 40 | --
Timing Chain Housing to the Camshaft Housings | 26 | 19 | --
Timing Chain Housing to the Block Bolts/Studs | 29 | 21 | --
Timing Chain Tensioner to Housing and Block | 10 | -- | 89
Throttle Body to the Intake Manifold | 10 | -- | 89
Thrust Plate to the Balance Shaft Housing | 13 | -- | 115
Transaxle To Block Bolt | 54 | 44 | --
Transaxle To Block Nut | 66 | 49 | --
Transaxle To Block Stud | 13 | -- | 115