For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch OFF.
2. Drain the oil from crankcase.
3. Remove the oil level switch electrical connector.
4. Remove the attaching bolt (1).
5. Remove the oil level switch (2).

### Installation Procedure

1. Install the oil level switch (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the attaching bolt (1).

Tighten
Tighten the attaching bolt to 10 N·m (7 lb ft).

3. Install the oil level switch electrical connector.
4. Refill the crankcase with engine oil.