For 1990-2009 cars

## Door Water Deflector Replacement Front

### Removal Procedure

A waterproof, clear, plastic deflector seals the door inner panel and prevents entry of water. Secure the inner panel to the deflector with waterproof adhesive. This allows the deflector to be peeled back in order to service the door components.

Important: Reseal the deflector with waterproof tape if the deflector becomes loose or damaged.

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector.

### Installation Procedure

1. Install the water deflector.
2. Insert the tabs at the bottom of the water deflector into the slots at the bottom of the door inner panel. Place the fastener holes in the deflector in their original position.
3. Install the door trim panel. Refer to Door Trim Panel Replacement .

## Door Water Deflector Replacement Rear

### Removal Procedure

A waterproof, clear, plastic deflector seals the door inner panel and prevents entry of water. Secure the inner panel to the deflector with waterproof adhesive. This allows the deflector to be peeled back in order to service the door components.

Important: Reseal the deflector with waterproof tape if the deflector becomes loose or damaged.

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the water deflector (1).

### Installation Procedure

1. Install the water deflector (1).
2. Insert the tabs at the bottom of the water deflector into the slots at the bottom of the door inner panel. Place the fastener holes in the deflector in their original position.
3. Install the door trim panel. Refer to Door Trim Panel Replacement .