For 1990-2009 cars

### Removal Procedure

1. Remove the outer belt sealing strip (1) on the door:

1.1. | Press the ratchet on the retainer (3) at the rear of the sealing strip (1).

1.2. | Lift to disengage the retainer (3).

2. Pull up on the sealing strip in order to release the strip from the clips (2).
3. Slide the sealing strip back in order to disengage the strip from the front of the door window frame molding.
4. Remove the sealing strip clips (2).

### Installation Procedure

1. Install the clips (2) to the outer belt sealing strip (1) on the door.
2. Slide the front of the sealing strip into the door frame molding.
3. Align the sealing strip clips (2) to the slots in the door. Engage the strip by pushing down until you hear an audible snap at each clip.