For 1990-2009 cars

# GAP BETWEEN DOOR TRIM PANEL & SIDE WINDOW DEFOGGER GRILLE

#### SUBJECT: GAP BETWEEN DOOR TRIM PANEL AND SIDE WINDOW DEFOGGER OUTLET GRILLE (APPLY ADHESIVE)

#### MODELS: 1992-94 OLDSMOBILE ACHIEVA

#### CONDITION:

SOME OWNERS MAY COMMENT ON A GAP BETWEEN THE DOOR TRIM PANEL AND THE SIDE WINDOW DEFOGGER OUTLET GRILLE.

#### CAUSE:

THE DOOR TRIM PANEL SKIN DELAMINATES FROM THE FOAM OR THE FOAM DELAMINATES FROM THE DOOR TRIM PANEL SUBSTRATE. ANOTHER POSSIBLE CAUSE COULD BE EXCESSIVE FOAM BUILD UP ON THE INBOARD SIDE OF THE DOOR TRIM PANEL.

#### CORRECTION:

1. REMOVE THE SIDE WINDOW DEFOGGER OUTLET GRILLE FROM THE DOOR TRIM PANEL.

2. INSPECT THE DOOR TRIM PANEL SKIN OR FOAM FOR DELAMINATION.

3. IF DELAMINATION HAS OCCURRED, APPLY LOCTITE(R) SUPER BONDER 495 ADHESIVE OR EQUIVALENT TO THE DOOR TRIM PANEL SKIN OR THE DOOR TRIM PANEL SUBSTRATE.

#### NOTE: THE DOOR PANEL SKIN OR FOAM MUST BE POSITIONED BEFORE THE ADHESIVE SETS (APPROXIMATELY 5 SECONDS).

4. INSTALL THE SIDE WINDOW DEFOGGER OUTLET GRILLE.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: T3466 LABOR TIME: 0.2 HR

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.